****

**City of Bastrop Inspection Requirements**



**International Plumbing Code (IPC)**



**NOTE: The commercial (C) and residential (R) energy code inspections as required by the International Energy Conservation Code (IECC) are incorporated in the IPC inspections listed and are preceded by the letters IECC.**

107.2 Required inspections and testing

Underground inspection shall be made after trenches or ditches are excavated and bedded, piping installed, and before backfill is put in place. Where excavated soil contains rocks, broken concrete, frozen chunks, and other rubble that would damage or break the piping or cause corrosive action, clean backfill shall be on the job site

Rough-in inspection shall be made after the roof, framing, fireblocking, firestopping, draftstopping, and bracing are in place and all storm and water distribution piping is roughed-in and prior to the installation of wall or ceiling membranes

IECC C105.2.3

Verify the type of insulation, *R*-values, protection required, controls and heat traps as required

IECC R105.2.3

Verify compliance as to types of insulation and corresponding *R*-values and protection and required controls

Final inspection shall be made after the building is complete, all plumbing fixtures are in place and properly connected, and the structure is ready for occupancy

\*The code official is authorized to make or require other inspections of any construction work to ascertain compliance

**City of Bastrop Inspections**

* Plumbing Rough
* Plumbing Underground Sewer
* Pluming Underground Water
* Plumbing Above Ceiling (C)
* Plumbing copper/PEX
* Plumbing Top Out
* Grease Trap Inspection (C)
* Plumbing Gas Test
* Med Gas (C)
* Fire Line Rough (C)
* Plumbing Gas Meter Release
* CSI
* Plumbing Final